Helicopter Programming Guide

Model Name:  BELT-CP
Model Number:  
	
	THRO
	AILE
	ELEV
	RUDD
	GEAR
	PITCH
	AUX2

	REVERSE SW [R/N]
	R   /   N
	R   /   N
	R   /   N
	R   /   N
	R   /   N
	R   /   N
	R   /   N

	SUB TRIM
	N
	R
	R
	R
	N
	N
	R

	TRAVEL ADJUST
	H     100%
	L     100%
	U     100%
	L     100%
	+     100%
	H     100%
	H     100%

	
	L     100%
	R    100%
	D     100%
	R     100%
	-     100%
	L     100%
	L     100%


	THROTTLE CURVE
	
	P-LOW
	P-1
	P-MID
	P-3
	P-HIGH

	
	NORMAL
	0%
	15%
	45%
	60%
	80%

	
	STUNT 1
	0%
	INH
	50%
	INH
	100%

	
	STUNT 2
	0%
	INH
	50%
	INH
	100%

	THROTTLE HOLD
	ON    /    OFF
	POSITION

	
	
	INH


	PITCH CURVE
	
	P-LOW
	P-1
	P-MID
	P-3
	P-HIGH

	
	NORMAL
	25%
-2 o
	INH
	68%
+6 o
	INH
	100%
+10 o

	
	STUNT 1
	0%
	INH
	50%
	INH
	100%

	
	STUNT 2
	0%
	INH
	50%
	INH
	100%


	SWASH TYPE
	NORMAL
	90 CCPM
	120 CCPM
	180 CCPM


	
	AILE
	ELEV
	PITCH

	SWASH MIX
	+60%
	+60%
	-60%

	
	REV R   /   N
	REV R   /   N
	REV R   /   N

	
	D/R
	

	SWITCH SELECT
	GEAR
	

	
	FL-M
	


	
	
	CHANNEL
	SW
	+POS
	-POS
	OFFSET

	PROGRAM MIX
	MIX 1
	--
	ON
	0%
	0%
	0

	
	MIX 2
	--
	ON
	0%
	0%
	0

	
	MIX 3
	--
	ON
	0%
	0%
	0


	
	
	
	AILE
	ELEV
	RUDD

	DUAL RATE   /   EXPO
	0
	D / R
	100%
	100%
	100%

	
	
	EXP
	-50%
	LIN
	LIN

	
	1
	D / R
	%
	%
	%

	
	
	EXP
	%
	%
	%

	REVO MIX
	NORMAL
	UP
	0%

	
	
	DOWN
	0%

	
	STUNT
	UP
	0%

	
	
	DOWN
	0%


